\documentclass[17pt,xcolor=table]{beamer} 
\usepackage{beamerthemesplit}
\definecolor{sbhs}{RGB}{255,69,50}
\definecolor{sbhs1}{RGB}{255,97,73}
\setbeamercolor{structure}{fg=sbhs}
\setbeamercolor{alerted text}{fg=sbhs1}
\beamertemplateshadingbackground{blue!5}{yellow!10}
\logo{\includegraphics[height=1cm]{3t-logo.pdf}}
\usepackage{verbatim}
\usepackage{bm}
%\usepackage{txfonts}
\newenvironment{colorverbatim}[1][]
{
\color{blue}
}
{
\endverbatim
}

\begin{document}
\sffamily \bfseries
\title
[\scriptsize {Connecting SBHS to Computer}]
{Connecting SBHS to Computer}
\author [Rupak Rokade]
{\small Talk to a Teacher \\
http://spoken-tutorial.org \\
National Mission
  on Education 
  through ICT \\ 
http://sakshat.ac.in \\ [0.5cm]
  Rupak Rokade \\IIT Bombay \\ [0.4cm]
{\small 25 April 2012}}
\date{}
\begin{frame}
   \titlepage
\end{frame}

\begin{frame}[fragile]
\frametitle{Objectives}
In this spoken tutorial we will learn:
\begin{itemize}[<+-|alert@+>]
\item To set up physical communication between SBHS and computer 
\item To install USB driver
\end{itemize}
\end{frame}

\begin{frame}[fragile]
\frametitle{Prerequisites}
\hspace{1cm}SBHS with power cable and\\
\begin{center}
\includegraphics[width=0.25\linewidth]{sbhs.JPG}
\hspace{0.5cm}
$+$
\hspace{0.5cm}
\includegraphics[width=0.25\linewidth]{power-cable.JPG}\\
\vspace{10mm}
USB/RS232 communication cable\\
\includegraphics[width=0.25\linewidth]{usb-cabel.JPG}
\hspace{0.5cm}
OR
\hspace{0.5cm}
\includegraphics[width=0.25\linewidth]{serial-cabel.JPG}\\
\end{center}
\end{frame}



\begin{frame}
\frametitle{Prerequisites}
On a Windows machine
\begin{itemize}[<+-|alert@+>]
\item FTDI VCP USB driver
\item You may download it from:\\www.ftdichip.com/Drivers\\/VCP.htm
%\item Scroll down and choose the driver file for your OS
%\item I downloaded 32 bit 2.08.13 driver file for Windows
\end{itemize}
\end{frame}




\begin{frame}[fragile]
\frametitle{Setting up}
\begin{itemize}[<+-|alert@+>]
\item Computer and SBHS can be connected using a USB cable or RS232 cable. 
\item Identify the corresponding ports on Computer and SBHS
\end{itemize}
\end{frame}

\begin{frame}[fragile]
\frametitle{Setting up}
USB ports on computer back panel
\begin{center}
\includegraphics[width=0.7\linewidth]{comp-usb2.jpg}
\end{center}
\end{frame}

\begin{frame}[fragile]
\frametitle{Setting up}
Serial port on computer back panel
\begin{center}
\includegraphics[width=0.7\linewidth]{comp-serial.jpg}
\end{center}
\end{frame}

\begin{frame}[fragile]
\frametitle{Setting up}
USB and Serial port on SBHS
\begin{center}
\includegraphics[width=0.7\linewidth]{sbhs-ports.jpg}
\end{center}
\end{frame}

\begin{frame}[fragile]
\frametitle{Setting up}
Jumpers to be used to select USB or RS232 port
\begin{center}
\includegraphics[width=0.7\linewidth]{jumpers.jpg}
\end{center}
\end{frame}


\begin{frame}[fragile]
\frametitle{Setting up}
Jumper connectors on SBHS
\begin{center}
\includegraphics[width=0.7\linewidth]{jumper-connectors.jpg}
\end{center}
\end{frame}





\begin{frame}[fragile]
\frametitle{Setting up}
Jumpers connected to select USB port
\begin{center}
\includegraphics[width=0.7\linewidth]{jumper1n2-settings.jpg}
\end{center}
\end{frame}

\begin{frame}[fragile]
\frametitle{Setting up}
%\begin{itemize}
%\item Connect power cable to a 3 pin AC 230 Volt house hold socket and the SBHS
%\item Switch the mains power ON. There may or may not be a ON/OFF switch on the SMPS of the SBHS. 
%\item If the device is succesfully powerd, the display should turn ON
%\end{itemize}
Connect the power cable as shown
\begin{center}
\includegraphics[width=0.6\linewidth]{power-connection.jpg}
\end{center}
\end{frame}

\begin{frame}[fragile]
\frametitle{SBHS Display}
\begin{center}
\includegraphics[width=0.5\linewidth]{display.jpg}
\end{center}
Note that what is displayed on the display may vary from what is shown. But it should certainly not be blank.
\end{frame}



\begin{frame}[fragile]
\frametitle{USB connection}
Connect USB cable to SBHS and Computer as shown
\begin{center}
\includegraphics[width=0.7\linewidth]{usb-connection.JPG}
\end{center}
\end{frame}

\begin{frame}[fragile]
\frametitle{Setting up}
Always make sure that you 
\begin{itemize}
\item First connect the Power Cable and 
\item Then the USB cable. 
\end{itemize}
\end{frame}

\begin{frame}
\frametitle{Installing driver}
Download the driver installation guide from \\{\color{red}www.ftdichip.com}
\end{frame}


\begin{frame}[fragile]
\frametitle{Summary}
%In this tutorial, we have learnt how to,
\begin{enumerate}
\item Connect SBHS and computer 
\begin{itemize}
\item Choosing RS232/USB port
\item Jumper settings
\item Powering ON the SBHS
\end{itemize}
\item Install USB driver
\begin{itemize}
\item Downloading installation guide
\item Following the guide and installing the driver
\end{itemize}
\end{enumerate}
\end{frame}

\begin{frame}
\frametitle{About the Spoken Tutorial Project}
\begin{itemize}
\item Watch the video available at {\color{red} http://spoken-tutorial.org /What\_is\_a\_Spoken\_Tutorial}
\item It summarises the Spoken Tutorial project 
\item If you do not have good bandwidth, you can download and watch it
\end{itemize}
\end{frame}

\begin{frame}
\frametitle{Spoken Tutorial Workshops}The Spoken Tutorial Project Team 
\begin{itemize}
\item Conducts workshops using spoken tutorials
\item Gives certificates to those who pass an online test
\end{itemize}
For more details, please write to \\ {\color{red}contact@spoken-tutorial.org}

\end{frame}

\begin{frame}
\frametitle{Acknowledgements}
\begin{itemize}
\item Spoken Tutorial Project is a part of the Talk to a Teacher  project
\item It is supported by the National Mission on Education through  ICT, MHRD, Government of India
\item More information on this Mission is available at: \\ {\color{red} http://spoken-tutorial.org \\ /NMEICT-Intro}
\end{itemize}
\end{frame}


\end{document}
















\begin{frame}
\frametitle{About the contributor} 
\begin{itemize}
\item Rupak Rokade from IIT Bombay
\item Thank you for joining
\end{itemize}
\end{frame}





\begin{frame}
\frametitle{Installing driver}
To download guide for ftdi driver installation
\begin{enumerate}
\item Go to {\tt www.ftdichip.com}
\item Click on Drivers
\item In the dropdown menu, choose {\tt VCP Drivers}
\item Click on {\tt Installation Guides} link
\item Choose required OS document
\end{enumerate}
\end{frame}
